(module keyboard_parts:ALPS_PLATE (layer F.Cu) (tedit 59475B7C)
  (descr http://deskthority.net/wiki/File:Alps_Electric_--_spec_--_5454_31.pdf)
  (tags "ALPS, keyboard switch, SKCM, SKCL")
  (fp_text reference SW29 (at 0 0) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.2)) (justify mirror))
  )
  (fp_text value SW_PUSH (at 0 10.795) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -9.525 -9.525) (end -9.525 9.525) (layer F.SilkS) (width 0.15))
  (fp_line (start -9.525 9.525) (end 9.525 9.525) (layer F.SilkS) (width 0.15))
  (fp_line (start 9.525 9.525) (end 9.525 -9.525) (layer F.SilkS) (width 0.15))
  (fp_line (start 9.525 -9.525) (end -9.525 -9.525) (layer F.SilkS) (width 0.15))
  (pad "" np_thru_hole circle (at 0 6.624988 90) (size 2.54 2.54) (drill 2.54) (layers *.Cu))
  (pad 3 thru_hole circle (at 5.75 5.999988 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at 5.75 -5.999988 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole circle (at -5.75 2.5 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at -5.75 -2.5 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 -6.624988 90) (size 2.54 2.54) (drill 2.54) (layers *.Cu))
)
