(module ALPS-LEDONLY-FLIPPED (layer F.Cu) (tedit 5CF32778)
  (fp_text reference REF** (at 0 6.604) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value LED (at -5.334 5.842) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 5 -7) (end 7 -7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 7 -7) (end 7 -5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 5 7) (end 7 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 7 7) (end 7 5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7 5) (end -7 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7 7) (end -5 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -5 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7 -7) (end -7 -5) (layer Dwgs.User) (width 0.15))
  (pad 1 thru_hole circle (at -1.27 4.6) (size 2 2) (drill 1.2) (layers *.Cu B.Mask))
  (pad 2 thru_hole rect (at 1.27 4.6) (size 2 2) (drill 1.2) (layers *.Cu B.Mask))
)
