(module MX_Alps_Hybrid:MX-7U (layer F.Cu) (tedit 5B2135A8)
  (fp_text reference REF** (at 0 3.175) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 7U (at 0 -7.9375) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 5 -7) (end 7 -7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 7 -7) (end 7 -5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 5 7) (end 7 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 7 7) (end 7 5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7 5) (end -7 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7 7) (end -5 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -5 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7 -7) (end -7 -5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -66.675 -9.525) (end 66.675 -9.525) (layer Dwgs.User) (width 0.15))
  (fp_line (start 66.675 -9.525) (end 66.675 9.525) (layer Dwgs.User) (width 0.15))
  (fp_line (start -66.675 9.525) (end 66.675 9.525) (layer Dwgs.User) (width 0.15))
  (fp_line (start -66.675 9.525) (end -66.675 -9.525) (layer Dwgs.User) (width 0.15))
  (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask))
  (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask))
)
