(module KailhChoc-1.5U (layer F.Cu) (tedit 5C519AAD)
  (fp_text reference REF** (at 0 3.175) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 1.5U (at 0 -7.9375) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 5 -7) (end 7 -7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 7 -7) (end 7 -5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 5 7) (end 7 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 7 7) (end 7 5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7 5) (end -7 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7 7) (end -5 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -5 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7 -7) (end -7 -5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -14.2875 -9.525) (end 14.2875 -9.525) (layer Dwgs.User) (width 0.15))
  (fp_line (start 14.2875 -9.525) (end 14.2875 9.525) (layer Dwgs.User) (width 0.15))
  (fp_line (start 14.2875 9.525) (end -14.2875 9.525) (layer Dwgs.User) (width 0.15))
  (fp_line (start -14.2875 9.525) (end -14.2875 -9.525) (layer Dwgs.User) (width 0.15))
  (pad 2 thru_hole circle (at 0 -5.9) (size 2 2) (drill 1.2) (layers *.Cu B.Mask))
  (pad "" np_thru_hole circle (at 0 0) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 5 -3.8) (size 2 2) (drill 1.2) (layers *.Cu B.Mask))
  (pad "" np_thru_hole circle (at -5.5 0 48.1) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 5.5 0 48.1) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -5.22 4.2) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -1.27 4.7) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
  (pad 4 thru_hole rect (at 1.27 4.7) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
)
