(module ALPS-ISO-2 (layer F.Cu) (tedit 5E9BC7BD)
  (fp_text reference REF** (at 0 3.175) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value ALPS-ISO-2 (at 0 -7.9375) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -11.90625 19.05) (end -11.90625 0) (layer Dwgs.User) (width 0.15))
  (fp_line (start -11.90625 0) (end -16.66875 0) (layer Dwgs.User) (width 0.15))
  (fp_line (start 5 -7) (end 7 -7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 7 -7) (end 7 -5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 5 7) (end 7 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 7 7) (end 7 5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7 5) (end -7 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7 7) (end -5 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -5 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7 -7) (end -7 -5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -16.66875 -19.05) (end 11.90625 -19.05) (layer Dwgs.User) (width 0.15))
  (fp_line (start 11.90625 -19.05) (end 11.90625 19.05) (layer Dwgs.User) (width 0.15))
  (fp_line (start -11.90625 19.05) (end 11.90625 19.05) (layer Dwgs.User) (width 0.15))
  (fp_line (start -16.66875 -19.05) (end -16.66875 0) (layer Dwgs.User) (width 0.15))
  (fp_line (start 7 -7) (end 5 -7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.525 -9.525) (end 9.525 -9.525) (layer Dwgs.User) (width 0.15))
  (fp_line (start 7 5) (end 7 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.525 -9.525) (end 9.525 9.525) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7 -7) (end -7 -5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.525 -9.525) (end -9.525 9.525) (layer Dwgs.User) (width 0.15))
  (fp_line (start 7 7) (end 5 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -5 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7 7) (end -5 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 7 -5) (end 7 -7) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7 5) (end -7 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.525 9.525) (end -9.525 9.525) (layer Dwgs.User) (width 0.15))
  (pad "" np_thru_hole circle (at -6.985 11.938) (size 3.048 3.048) (drill 3.048) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -6.985 -11.938) (size 3.048 3.048) (drill 3.048) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 8.255 11.938) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 8.255 -11.938) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 4 -2.5 270) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask))
  (pad 2 thru_hole circle (at 4.5 2.5 270) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask))
)
