(module MXOnly-2U-VerticalStabilizers-NoSwitch (layer F.Cu) (tedit 5EACBD1E)
  (fp_text reference REF** (at 0 3.175) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value MXOnly-2U-VerticalStabilizers-NoSwitch (at 0 -0.5) (layer Dwgs.User) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -9.525 -19.05) (end 9.525 -19.05) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.525 19.05) (end -9.525 19.05) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.525 19.05) (end 9.525 -19.05) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.525 19.05) (end -9.525 -19.05) (layer Dwgs.User) (width 0.15))
  (fp_text user 2U (at -7.9375 0 270) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "" np_thru_hole circle (at -6.985 -11.938 180) (size 3.048 3.048) (drill 3.048) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -6.985 11.938 90) (size 3.048 3.048) (drill 3.048) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 8.255 11.938 90) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 8.255 -11.938 90) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
)
