(module MX-6U-ReversedStabilizers (layer F.Cu) (tedit 5A9F50B1)
  (fp_text reference REF** (at 9.525 3.175) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 6U (at 9.525 -7.9375) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 14.525 -7) (end 16.525 -7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 16.525 -7) (end 16.525 -5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 14.525 7) (end 16.525 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 16.525 7) (end 16.525 5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 2.525 5) (end 2.525 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 2.525 7) (end 4.525 7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 4.525 -7) (end 2.525 -7) (layer Dwgs.User) (width 0.15))
  (fp_line (start 2.525 -7) (end 2.525 -5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -57.15 -9.525) (end 57.15 -9.525) (layer Dwgs.User) (width 0.15))
  (fp_line (start 57.15 -9.525) (end 57.15 9.525) (layer Dwgs.User) (width 0.15))
  (fp_line (start -57.15 9.525) (end 57.15 9.525) (layer Dwgs.User) (width 0.15))
  (fp_line (start -57.15 9.525) (end -57.15 -9.525) (layer Dwgs.User) (width 0.15))
  (pad 2 thru_hole oval (at 12.025 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask))
  (pad 2 thru_hole circle (at 12.065 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask))
  (pad 1 thru_hole oval (at 5.715 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask))
  (pad "" np_thru_hole circle (at 9.525 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 7.025 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask))
  (pad 3 thru_hole circle (at 8.255 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
  (pad 4 thru_hole rect (at 10.795 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
  (pad "" np_thru_hole circle (at 4.445 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 14.605 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -47.625 6.985) (size 3.048 3.048) (drill 3.048) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 47.625 6.985) (size 3.048 3.048) (drill 3.048) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -47.625 -8.255) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 47.625 -8.255) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
)
